{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"images":1,"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":25,"n_cols":10,"rows_kept":25,"merged":[[1,5,1,7],[1,8,1,9],[2,1,3,1],[2,2,2,9],[12,2,13,2],[12,3,13,3],[12,4,13,4],[12,5,13,5],[12,6,13,6],[12,7,13,7],[12,8,13,8],[12,9,13,9]],"flags":["formulas_cached_only"]}
[]
[{"$nulls":8}," WZD 25.1 "]
[null,null,"Consolis Design Model (CDM)"]
[null,null,8,7,6,5,4,3,2,1]
[null,"1.0. Podstawy do projektowania:"]
[null,"- klasa ppoż i ekspozycji","x"]
[null,"- obciążenia","x"]
[null,"- uwzględnienie obciążeń sejsmicznych \n(np. tereny górnicze)","x","x"]
[null,"2.0. Obliczenia konstrukcji:"]
[null,"- obliczenia statyczne","x","x","x"]
[null,"- sprawdzenie stateczności obiektu","x","x","x"]
[null,"- siły przekrojowe dla wszystkich elementów","x","x","x"]
[null,"- wymiarowanie elementów (pkt.2.5 DRA)",null,"x","x","x","x","x"]
[null,"- wytyczne do zbrojenia (pkt. 3.4 DRA)"]
[null,"3.0. Rysunki konstrukcji:"]
[null,"- schemat konstrukcji","x","x","x"]
[null,"- detale montażowe",null,"x","x","x"]
[null,"- schemat złożeniowy (montażowy)",null,"x","x","x","x"]
[null,"- rysunki warsztatowe",null,"x","x","x","x","x","x"]
[]
[null,"Produkcja i dostawa",null,"x","x","x","x","x","x","x"]
[]
[]
[null,"Legenda "]
[null,"\"X\"-po stronie Consolis"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}